L20 Doors/ Shutters/ Hatches

610 Roller shutter doors 

Specification Text 

Manufacturer: HVP Security Shutters Ltd, 4 Grace Road West, Marsh Barton, Exeter, EX2 8PU. Tel: 01392 270 218. Fax: 01392 278 548. Email: info@hvpshutters.co.uk Website: www.hvpshutters.co.uk

Product reference: Armourshield Roller Grille
 

Arrangement: Vertically operating roller grille for face/reveal fixing.


Construction: Manufactured from 6mm or 8mm solid steel bars, press formed into the grille profile. Grille bars locked together with pressed steel clips; double extruded aluminium bottom rail with weather seal (6mm grille) or roll-formed steel bottom rail (8mm grille); extruded aluminium guides with weather seals: 53mm x 22mm (6mm grille) or 75mm x 27mm (8mm grille). 

Canopy: Aluminium sheet folded to enclose the rear of the shutter barrel and curtain assembly.


Finish as delivered: Zinc plated in silver or gold colour, Polyester Powder Coated, or stainless steel (8mm grille only).

Operation: Electric operation by integral tubular motor with manual override facility. Safety brake fitted when required to comply with BS EN 13241:2003-1 (HVP Security Shutters’ general policy is to fit a safety brake unless specified otherwise).


Locking options: Bottom rail central key lock. Electrically operated grilles are generally self-locking. 

Other requirements:
