L20 Doors/ Shutters/ Hatches

610 Roller shutter doors 

Specification Text 

Manufacturer: HVP Security Shutters Ltd, 4 Grace Road West, Marsh Barton, Exeter, EX2 8PU. Tel: 01392 270 218. Fax: 01392 278 548. Email: info@hvpshutters.co.uk Website: www.hvpshutters.co.uk

Product reference: K77 / K55 Aluminium Roller Shutter
 

Arrangement: Vertically operating roller grille for face/reveal fixing.


Construction: Curtain manufactured from foam-filled aluminium lath profile 77mm high x 19mm thick (K77) or 55mm high x 13.5mm thick (K55). For applications that require light or vision to pass through the door, non insulated punched and glazed slats can be incorporated into the door curtain (K77 only).

Canopy (optional): Roll formed aluminium in two sections; top and bottom boxes. Bottom box removable for installation and maintenance and chamfered at 45°. The shutter box is assembled on die cast aluminium endplates.
Finish as delivered: Polyester Powder Coated White or Dark Brown finish as standard to all exposed parts; range of other colours available, including textured woodgrain finishes.
Operation: Electric operation by internal tubular motor with manual override facility. Safety Brake fitted when required to comply with BS EN 13241:2003-1 (HVP Security Shutters’ general policy is to fit a safety brake unless specified otherwise).


Locking options: Electrically operated grilles are generally self-locking. 

For additional security HVP Security Shutters recommends guide pin locks or a ground padlocking unit combined with a motor isolator box.


Other requirements:
