L20 Doors/ Shutters/ Hatches

610 Roller shutter doors 

Specification Text 

Manufacturer: HVP Security Shutters Ltd, 4 Grace Road West, Marsh Barton, Exeter, EX2 8PU. Tel: 01392 270 218. Fax: 01392 278 548. Email: info@hvpshutters.co.uk Website: www.hvpshutters.co.uk

Product reference: K80 Aluminium Punched Roller Shutter
 

Arrangement: Vertically operating roller grille for face/reveal fixing.


Construction: Curtain manufactured from punched aluminium lath profile 80mm high x 19mm thick lath. For applications that require light or vision to pass through the door. Glazed slats can be incorporated into the door curtain if required.

Canopy (optional): Roll formed aluminium in two sections; top and bottom boxes. Bottom box removable for installation and maintenance and chamfered at 45°. The shutter box is assembled on die cast aluminium endplates.
Finish as delivered: Polyester Powder Coated White, Black, Anthracite grey or Dark Brown finish as standard to all exposed parts; range of other colours available, including textured woodgrain finishes.
Operation: Electric operation by internal tubular motor with manual override facility. Safety Brake fitted when required to comply with BS EN 13241:2003-1 (HVP Security Shutters’ general policy is to fit a safety brake unless specified otherwise).


Locking options: Electrically operated grilles are generally self-locking. 

For additional security HVP Security Shutters recommends guide pin locks or a ground padlocking unit combined with a motor isolator box.


Other requirements:
