L20 Doors/ Shutters/ Hatches

610 Roller shutter doors 

Specification Text 

Manufacturer: HVP Security Shutters Ltd, 4 Grace Road West, Marsh Barton, Exeter, EX2 8PU. Tel: 01392 270 218. Fax: 01392 278 548. Email: info@hvpshutters.co.uk Website: www.hvpshutters.co.uk

Product reference: SeceuroVision 800 Roller Shutter
 

Arrangement: Vertically operating roller grille for face/reveal fixing.


Construction: Manufactured from 80mm aluminium lath extruded section with 150 x 55mm cut-outs; Extruded aluminium bottom rail with optional bottom rail weather seal; Extruded aluminium guides 90mm wide x 34mm deep with an integral box section for reinforcement and to facilitate fixing. High density 4mm pile brush seals for quiet and smooth operation. Optional glazing comprising of 1.5mm thick polycarbonate glass strips.

Canopy (optional): Roll formed aluminium in two sections; top and bottom boxes. Bottom box removable for installation and maintenance and chamfered at 45°. The shutterbox is assembled on die cast aluminium endplates.
Finish as delivered: Polyester Powder Coated White or Dark Brown as standard. Complete shutter can be powder coated to any RAL colour (some non-standard colours may increase the delivery time).
Operation: Electric operation by internal tubular motor with manual override facility. Safety brake fitted when required to comply with BS EN 13241:2003-1 (HVP Security Shutters’ general policy is to fit a safety brake unless specified otherwise).


Locking options: Electrically operated grilles are generally self-locking. For additional security HVP Security Shutters recommends guide pin locks or a ground padlocking unit combined with a motor isolator box.


Other requirements:
