L20 Doors/ Shutters/ Hatches

610 Roller shutter doors 

Specification Text 

Manufacturer: HVP Security Shutters Ltd, 4 Grace Road West, Marsh Barton, Exeter, EX2 8PU. Tel: 01392 270 218. Fax: 01392 278 548. Email: info@hvpshutters.co.uk Website: www.hvpshutters.co.uk

Product reference: SeceuroVision 900 Roller Grille
Arrangement: Vertically operating roller grille for face/reveal fixing.


Construction: Manufactured from extruded aluminium bars and links with 150mm x 70mm vision openings as standard or optional 75mm x 70mm vision openings; Extruded aluminium bottom rail with optional bottom rail weather seal; Aluminium guides 60 to 90 mm wide and 27 to 34mm deep (depending on canopy box size) with high density 4mm or 7mm pile brush for quiet and smooth operation.

Canopy (optional): Roll formed aluminium in two sections; top and bottom boxes. Bottom box removable for installation and maintenance and chamfered at 45°. The shutterbox is assembled on die cast aluminium endplates.
Finish as delivered: Anodised aluminium as standard. Complete shutter can be powder coated to any RAL colour (some non-standard colours may increase the delivery time).

Box and guides white or dark brown as standard, or can be powder coated to match the curtain.
Operation: Electric operation by internal tubular motor with manual override facility. Safety brake fitted when required to comply with BS EN 13241:2003-1 (HVP Security Shutters’ general policy is to fit a safety brake unless specified otherwise).


Locking options: Electrically operated grilles are generally self-locking. For additional security HVP Security Shutters recommends guide pin locks or a ground padlocking unit combined with a motor isolator box.


Other requirements:
