L20 Specification Texts FlexiGlide Sliding Folding Shutters

1. Barrier 

2. Classic Chainlink

3. Protector

4. Vision Air

5. Vision Glass

6. Vision Guard

L20 Doors/ Shutters/ Hatches

610 Roller shutter doors 

Specification Text 

Manufacturer: HVP Security Shutters Ltd, 4 Grace Road West, Marsh Barton, Exeter, EX2 8PU. Tel: 01392 270 218. Fax: 01392 278 548. Email: info@hvpshutters.co.uk Website: www.hvpshutters.co.uk. 

Product reference: FlexiGlide Barrier Sliding Folding Shutter.

Arrangement: Horizontally operated top hung sliding folding shutter.

Construction: The Barrier incorporates 51mm high truss-like plates at the top and bottom of the closure. Constructed of 102mm wide x 1.5mm thick aluminium plates that slide over 8mm rods on 89mm centres in an alternating pattern. Plate height is indicated by model number (Sentry 33 - 3” plates, Sentry 1515 - 15” plates).
Track: The overhead track is 33mm wide x 46mm high and takes 29mm diameter roller trolleys. The rollers bear on a 7mm thick aluminium surface within the track. Track curves, where indicated, have 254mm or 356mm radii. A custom radius track is available as an option.

Finish as delivered: Standard factory finishes are 10 micron clear anodizing, K1285 (white), K70632 (light bronze), K71232 (medium bronze) or K90421 (black) Duracron acrylic paint. The complete shutter can be powder coated to any RAL colour (some non-standard colours may increase the delivery time).
Operation: Manual operation.

Locking Options: The grille incorporates vertical posts at regular intervals fabricated from rectangular tubing 33mm x 62mm. Posts with floor bolts include dust free, stainless-top floor sockets. Lead and trailing end posts are cylinder controlled lock stiles with self-adjusting, cold rolled steel floor bolts and top bolts through the top of the track into the support. Intermediate locking posts with cold rolled steel floor bolts are supplied for (up to) every 3048mm of curtain. Bi-part assemblies are supplied as required. One locking post has a hook-bolt deadlock activated by keyed or thumb-turn cylinders. A second intermediate locking post with a steel floor bolt includes a full height channel to accept the hook-bolt deadlock. 

Weight and Stacking: Grille weight is expressed in kg/square metre of clear opening. Barrier – 7.3 kg/square metre. Minimum stacking is 87.5mm/metre of opening plus 89mm per locking member. The grille support must be able to carry the weight of a fully stacked door at any point along its length. Design structural support to carry the total weight / the total stacking.

Other requirements:
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Product reference: FlexiGlide Classic Chainlink Sliding Folding Shutter.

Arrangement: Horizontally operated top hung sliding folding shutter.

Construction: Manufactured using 51mm high truss-like plates at the top and bottom of the closure. Constructed of 8mm diameter vertical rods on 89mm centres linked by flat horizontal bars 3mm x 16mm x 197mm. Bars are vertically spaced every 305mm with 11mm diameter sleeves over alternating rods.
Track: The overhead track is 33mm wide x 46mm high and takes 29mm diameter roller trolleys. The rollers bear on a 7mm thick aluminium surface within the track. Track curves, where indicated, have 254mm or 356mm radii. A custom radius track is available as an option.

Finish as delivered: Standard factory finishes are: 10 micron clear anodizing, K1285 (white), K70632 (light bronze), K71232 (medium bronze), or K90421 (black) Duracron acrylic paint. Powder coating is not recommended.

Operation: Manual operation.

Locking Options: The grille incorporates vertical posts at regular intervals fabricated from rectangular tubing 33mm x 62mm. Posts with floor bolts include dust free, stainless-top floor sockets. Lead and trailing end posts are cylinder controlled lock stiles with self-adjusting, cold rolled steel floor bolts and top bolts through the top of the track into the support. Intermediate locking posts with cold rolled steel floor bolts are supplied for (up to) every 3048mm of curtain. Bi-part assemblies are supplied as required. One locking post has a hook-bolt deadlock activated by keyed or thumb-turn cylinders. A second intermediate locking post with a steel floor bolt includes a full height channel to accept the hook-bolt deadlock. 

Weight and Stacking: Grille weight is expressed in kg/square metre of clear opening. Classic Chainlink - 5.9 kg/square metre. Minimum stacking is 87.5mm/metre of opening plus 89mm per locking member. The grille support must be able to carry the weight of a fully stacked door at any point along its length. Design structural support to carry the total weight / the total stacking.

Other requirements:
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Product reference: FlexiGlide Protector Sliding Folding Shutter.

Arrangement: Horizontally operated top hung sliding folding shutter.

Construction: Constructed of 152mm wide by 1.83mm thick full height aluminium panels, framed by full height butt hinges on 178mm centres.


Track: The overhead track is 33mm wide x 46mm high and takes 29mm diameter roller trolleys. The rollers bear on a 7mm thick aluminium surface within the track. Track curves, where indicated, have 254mm or 356mm radii. A custom radius track is available as an option.

Finish as delivered: Standard factory finishes are 10 micron clear anodizing, K1285 (white), K70632 (light bronze), K71232 (medium bronze) or K90421 (black) Duracron acrylic paint. The complete shutter can be powder coated to any RAL colour (some non-standard colours may increase the delivery time).

Operation: Manual operation.

Locking Options: The grille incorporates vertical posts at regular intervals fabricated from rectangular tubing 33mm x 62mm. Posts with floor bolts include dust free, stainless-top floor sockets. Lead and trailing end posts are cylinder controlled lock stiles with self-adjusting, cold rolled steel floor bolts and top bolts through the top of the track into the support. Intermediate locking posts with cold rolled steel floor bolts are supplied for (up to) every 3048mm of curtain. Bi-part assemblies are supplied as required. One locking post has a hook-bolt deadlock activated by keyed or thumb-turn cylinders. A second intermediate locking post with a steel floor bolt includes a full height channel to accept the hook-bolt deadlock. 

Weight and Stacking: Grille weight is expressed in kg/square metre of clear opening. Protector – 10.7 kg/square metre. Minimum stacking is 87.5mm/metre of opening plus 89mm per locking member. The grille support must be able to carry the weight of a fully stacked door at any point along its length. Design structural support to carry the total weight / the total stacking.

Other requirements:
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Product reference: FlexiGlide Vision Air Sliding Folding Shutter.

Arrangement: Horizontally operated top hung sliding folding shutter.

Construction: Constructed of 152mm wide x 1.83mm thick full height aluminium panels. Panels are framed by full height butt hinges on 178mm centres. Panels are perforated by 6mm x 32mm oblong slots in evenly spaced columns and staggered rows. Alternatively, they are perforated by 6mm diameter holes in a 4.76mm staggered pattern. The Vision Air incorporates 102mm high truss-like plates at the top and bottom of the closure.

Track: The overhead track is 33mm wide x 46mm high and takes 29mm diameter roller trolleys. The rollers bear on a 7mm thick aluminium surface within the track. Track curves, where indicated, have 254mm or 356mm radii. A custom radius track is available as an option.

Finish as delivered: Standard factory finishes are 10 micron clear anodizing, K1285 (white), K70632 (light bronze), K71232 (medium bronze) or K90421 (black) Duracron acrylic paint. The complete shutter can be powder coated to any RAL colour (some non-standard colours may increase the delivery time).

Operation: Manual operation.

Locking Options: The grille incorporates vertical posts at regular intervals fabricated from rectangular tubing 33mm x 62mm. Posts with floor bolts include dust free, stainless-top floor sockets. Lead and trailing end posts are cylinder controlled lock stiles with self-adjusting, cold rolled steel floor bolts and top bolts through the top of the track into the support. Intermediate locking posts with cold rolled steel floor bolts are supplied for (up to) every 3048mm of curtain. Bi-part assemblies are supplied as required. One locking post has a hook-bolt deadlock activated by keyed or thumb-turn cylinders. A second intermediate locking post with a steel floor bolt includes a full height channel to accept the hook-bolt deadlock. 

Weight and Stacking: Grille weight is expressed in kg/square metre of clear opening. Vision Air - 10.7 kg/square metre. Minimum stacking is 87.5mm/metre of opening plus 89mm per locking member. The grille support must be able to carry the weight of a fully stacked door at any point along its length. Design structural support to carry the total weight / the total stacking.

Other requirements:
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Product reference: FlexiGlide Vision Glass Sliding Folding Shutter.

Arrangement: Horizontally operated top hung sliding folding shutter.

Construction: Constructed from 152mm wide by 3.2mm thick tempered glass or self-extinguishing Lexan® (or equiv.) panels protected by co-extruded neoprene and PVC gaskets. Aluminium panels, framed by full height butt hinges on 178mm centres. The Vision Glass incorporates 102mm high truss-like plates at the top and bottom of the closure.

Track: The overhead track is 33mm wide x 46mm high and takes 29mm diameter roller trolleys. The rollers bear on a 7mm thick aluminium surface within the track. Track curves, where indicated, have 254mm or 356mm radii. A custom radius track is available as an option.

Finish as delivered: Standard factory finishes are 10 micron clear anodizing, K1285 (white), K70632 (light bronze), K71232 (medium bronze) or K90421 (black) Duracron acrylic paint. The complete shutter can be powder coated to any RAL colour (some non-standard colours may increase the delivery time).

Operation: Manual operation.

Locking Options: The grille incorporates vertical posts at regular intervals fabricated from rectangular tubing 33mm x 62mm. Posts with floor bolts include dust free, stainless-top floor sockets. Lead and trailing end posts are cylinder controlled lock stiles with self-adjusting, cold rolled steel floor bolts and top bolts through the top of the track into the support. Intermediate locking posts with cold rolled steel floor bolts are supplied for (up to) every 3048mm of curtain. Bi-part assemblies are supplied as required. One locking post has a hook-bolt deadlock activated by keyed or thumb-turn cylinders. A second intermediate locking post with a steel floor bolt includes a full height channel to accept the hook-bolt deadlock. 

Weight and Stacking: Grille weight is expressed in kg/square metre of clear opening. Vision Glass - 12.2 kg/square metre (tempered glass) or 10.7 kg/square metre (Lexan®). Minimum stacking is 87.5mm/metre of opening plus 89mm per locking member. The grille support must be able to carry the weight of a fully stacked door at any point along its length. Design structural support to carry the total weight / the total stacking.

Other requirements:
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Product reference: FlexiGlide Vision Guard Sliding Folding Shutter.

Arrangement: Horizontally operated top hung sliding folding shutter.

Construction: Constructed of 152mm wide x 19mm high truss-like horizontal members spaced at 305mm vertical intervals. The panel centreline consists of 11mm diameter tubing over a full height, concealed 8mm diameter rod. The panels are framed on 178mm centres.


Track: The overhead track is 33mm wide x 46mm high and takes 29mm diameter roller trolleys. The rollers bear on a 7mm thick aluminium surface within the track. Track curves, where indicated, have 254mm or 356mm radii. A custom radius track is available as an option.

Finish as delivered: Standard factory finishes are 10 micron clear anodizing, K1285 (white), K70632 (light bronze), K71232 (medium bronze) or K90421 (black) Duracron acrylic paint. The complete shutter can be powder coated to any RAL colour (some non-standard colours may increase the delivery time).

Operation: Manual operation.

Locking Options: The grille incorporates vertical posts at regular intervals fabricated from rectangular tubing 33mm x 62mm. Posts with floor bolts include dust free, stainless-top floor sockets. Lead and trailing end posts are cylinder controlled lock stiles with self-adjusting, cold rolled steel floor bolts and top bolts through the top of the track into the support. Intermediate locking posts with cold rolled steel floor bolts are supplied for (up to) every 3048mm of curtain. Bi-part assemblies are supplied as required. One locking post has a hook-bolt deadlock activated by keyed or thumb-turn cylinders. A second intermediate locking post with a steel floor bolt includes a full height channel to accept the hook-bolt deadlock. 

Weight and Stacking: Grille weight is expressed in kg/square metre of clear opening. Vision Guard – 7.3 kg/square metre. Minimum stacking is 87.5mm/metre of opening plus 89mm per locking member. The grille support must be able to carry the weight of a fully stacked door at any point along its length. Design structural support to carry the total weight / the total stacking.

Other requirements:

